{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":12,"n_cols":10,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["物料代码","物料名称","检验项目编码","检验项目名称","检验方法","检验属性","设计最大值","设计最小值","单位","启用(是否)"]
["8S10010",{"$f":"IF(A2=\"\",\"\",VLOOKUP(A:A,[1]料号维护顺序!B:J,2,0))","v":"支架左侧板"},"A001","包装外箱标签需包括厂商名称、订单号、料号、品名、材质、数量","目测","包装防护",null,null,null,"是"]
["8S10010",{"$f":"IF(A3=\"\",\"\",VLOOKUP(A:A,[1]料号维护顺序!B:J,2,0))","v":"支架左侧板"},"A002","包装箱需整洁、内部物料摆放须与WPI要求一致","目测","包装防护",null,null,null,"是"]
["8S10010",{"$f":"IF(A4=\"\",\"\",VLOOKUP(A:A,[1]料号维护顺序!B:J,2,0))","v":"支架左侧板"},"A003","检查尾数箱的实际数量是否与标签标识一致","目测","包装防护",null,null,null,"是"]
["8S10010",{"$f":"IF(A5=\"\",\"\",VLOOKUP(A:A,[1]料号维护顺序!B:J,2,0))","v":"支架左侧板"},"B001","外观不可油污、变形、缺口或破损等异常、颜色与图纸标注一致","目测","外观",null,null,null,"是"]
["8S10010",{"$f":"IF(A6=\"\",\"\",VLOOKUP(A:A,[1]料号维护顺序!B:J,2,0))","v":"支架左侧板"},"B002","与标准样比对无显著差异色差,与样品目检无显著差异\n(E<=2)","目测","外观",null,null,null,"是"]
["8S10010",{"$f":"IF(A7=\"\",\"\",VLOOKUP(A:A,[1]料号维护顺序!B:J,2,0))","v":"支架左侧板"},"C001","表面有害物质如何RoHS2.0、REACH法规要求","委外","有害物质",null,null,null,"是"]
["8S10010",{"$f":"IF(A8=\"\",\"\",VLOOKUP(A:A,[1]料号维护顺序!B:J,2,0))","v":"支架左侧板"},"D001","353.70 +0.50/-0.40 mm","卡尺","尺寸",354.2,353.3,"mm","是"]
["8S10010",{"$f":"IF(A9=\"\",\"\",VLOOKUP(A:A,[1]料号维护顺序!B:J,2,0))","v":"支架左侧板"},"D002",">183.00 mm","卡尺","尺寸",999999,183.01,"mm","是"]
["8S10010",{"$f":"IF(A10=\"\",\"\",VLOOKUP(A:A,[1]料号维护顺序!B:J,2,0))","v":"支架左侧板"},"D003","与水位检测PCB盖实配","实配","外观",null,null,null,"是"]
["8S10010",{"$f":"IF(A11=\"\",\"\",VLOOKUP(A:A,[1]料号维护顺序!B:J,2,0))","v":"支架左侧板"},"E001","≥540g","电子秤","重量",999999,540,"g","是"]
["8S10010",{"$f":"IF(A12=\"\",\"\",VLOOKUP(A:A,[1]料号维护顺序!B:J,2,0))","v":"支架左侧板"},"F001","气味：参照《零部件气味管控计划》",null,"性能",null,null,null,"是"]